****

**COLLEGE OF ENGINEERING & TECHNOLOGY**

**Department: Electronics & Communication**

**Alamein Campus**

**Name of Students:** Mohamed Maher, Zeyad Rashwan, Abdelrahman Ahmad, Ammar Eliwa, Youssef Hassaenin, Mazen Seyam, Alaa Abada

**Title of Report:** Design and Development of a Cartesian 3D printer

**Submitted to:** Dr. Ahmad Hany

**Course name:** Automatic Control Systems EE41

## **Table of Contents**

1. **Title Page ........................................................... Page 1**
2. **Abstract ............................................................ Page 2**
3. **Table of Contents .............................................. Page 3**
4. **Introduction .................................................... Page 4**
5. **Components .................................................... Page 5**
6. **Design and Assembly ....................................... Page 6-8**
7. **Testing and Results ........................................ Page 9**
8. **Challenges and Solutions .................................. Page 10**
9. **Conclusion and Future Work ............................. Page 11**
10. **References .................................................... Page 12**

## **Abstract**

Plastic pollution, particularly from PET #1 plastic bottles, is one of the most pressing environmental challenges of our time. The PET Plastic Filament Maker aims to address this issue by transforming waste into valuable 3D printing filament.

This innovative machine combines mechanical, electrical, and software components to recycle plastic bottles efficiently. Utilizing components such as the Clarity Ender Ten Hot End, Arduino Mega, RAMPS 1.4, and 3D-printed parts, the project demonstrates a cost-effective, sustainable solution to repurposing plastic waste. The machine operates by shredding PET bottles, heating the plastic to a molten state, and extruding it into filament suitable for 3D printing applications.

Through rigorous testing and iterative design, the filament maker has achieved a consistent diameter of 1.75 mm, meeting industry standards. This report outlines the development process, highlighting the challenges faced, solutions implemented, and future work required to enhance the machine’s capabilities. By empowering individuals and communities to recycle PET bottles into filament, this project contributes to a circular economy and promotes environmental sustainability.

The following pages provide a detailed breakdown of the components, assembly process, and performance of the PET Plastic Filament Maker.

## **Introduction**

Plastic waste, particularly PET bottles, is a significant environmental issue that continues to threaten ecosystems and contribute to pollution. These bottles, widely used for beverages and other products, are often discarded irresponsibly, resulting in vast quantities of waste accumulating in landfills, oceans, and natural habitats. As global awareness of the environmental impact of plastic waste grows, finding innovative and effective recycling methods has become increasingly critical. One promising solution involves repurposing PET bottles into 3D printing filament—a process that not only reduces waste but also supports sustainability and promotes circular economies.

This report outlines the development of a filament maker machine designed to transform discarded PET bottles into reusable filament for 3D printing applications. By addressing the challenges of plastic waste through engineering and innovation, this project aims to bridge the gap between recycling and advanced manufacturing technologies. The machine offers a practical approach to recycling by converting a commonly wasted material into a valuable resource, aligning with global efforts to minimize environmental impact and encourage sustainable practices.

The primary objectives of this project were to design a cost-effective, easy-to-build machine using readily available components and to produce high-quality filament suitable for a wide range of 3D printing applications. These goals were set with the intention of making this technology accessible to individuals, educational institutions, and small businesses, thereby democratizing access to sustainable manufacturing solutions. By using inexpensive and widely available materials, the filament maker ensures that anyone interested in reducing their environmental footprint can participate in this innovative recycling process.

In addition to being economically viable, the filament maker machine was designed with simplicity and functionality in mind. It emphasizes ease of use, enabling users with minimal technical expertise to operate the machine efficiently. This design philosophy ensures that the technology can be adopted by a broad audience, including hobbyists, students, and professionals in various fields. Furthermore, producing high-quality filament was a critical focus to ensure compatibility with a range of 3D printers, thereby maximizing its practical applications.

The environmental benefits of this project extend beyond reducing the volume of plastic waste. By transforming PET bottles into 3D printing filament, the project contributes to reducing the demand for virgin plastic, which is energy-intensive to produce and often derived from non-renewable fossil fuels. Additionally, this initiative promotes a culture of sustainability and resourcefulness, inspiring individuals and organizations to rethink waste and adopt innovative recycling practices.

Ultimately, this report aims to provide a comprehensive overview of the filament maker machine's development process, from conceptualization and design to implementation and testing. It highlights the potential of engineering and innovation to address pressing environmental challenges and underscores the importance of accessible, practical solutions in fostering a sustainable future. Through this project, we hope to inspire further advancements in recycling technologies and demonstrate the immense potential of combining environmental stewardship with cutting-edge manufacturing techniques.

## **Components**

The machine was built using the following components:

* **Clarity Ender Ten Hot End**: Facilitates the melting and extrusion of PET plastic.
* **Arduino Mega**: Acts as the central processing unit, managing inputs and outputs.
* **RAMPS 1.4 Board**: Provides motor control and power management.
* **Stepper Motor NEMA 17**: Drives the filament extrusion and spooling mechanisms.
* **Driver A4988**: Controls the stepper motor with precision.
* **Smart Graphical LCD**: Displays system information and allows user interaction.
* **3D-Printed Parts**: Custom-designed components for structural and functional purposes.

### **Additional Materials**

* PET #1 plastic bottles, cleaned and prepared for shredding.
* Power supply unit to provide consistent voltage for all components.
* Standard wiring and connectors for reliable electrical connections.

## **Design and Assembly**

### **Step 1: Printing the Parts**

All structural and functional components were 3D printed using a standard FDM printer. The designs were optimized for durability, precision, and ease of assembly. PETG filament was chosen for its strength and heat resistance.

### **Step 2: Assembling the Bottom Build**

The base of the machine was assembled first, including:

* Mounting the power supply.
* Installing the Arduino Mega and RAMPS 1.4 board.
* Connecting the Smart Graphical LCD.

### **Step 3: Wiring**

All electrical components were connected using labeled connectors and standard wiring practices. Care was taken to secure wires and minimize the risk of disconnections or short circuits.

### **Step 4: Completing the Top Build**

The top section, including the Clarity Ender Ten Hot End, was installed. This section handles the heating and extrusion of the PET plastic. The hot end was calibrated to ensure consistent melting and flow of the plastic.

### **Step 5: Motor Spooler Assembly**

The motorized spooler, powered by the NEMA 17 stepper motor, was assembled to ensure consistent winding of the extruded filament. A tensioning mechanism was added to maintain uniformity.

### **Step 6: Adding the End of the Tunnel**

A guide mechanism was added to direct the extruded filament smoothly onto the spooler. This step ensured that the filament maintained a consistent diameter during the spooling process.

### **Step 7: SD Card and Prep**

An SD card was configured with the necessary firmware to control the machine’s operations. The system was then tested for functionality and prepared for filament production. Additional preheating and calibration steps were performed to optimize performance.

## **Testing and Results**

The machine was tested with PET bottles to evaluate its performance. Key observations include:

### **Filament Quality**

The produced filament exhibited a consistent diameter of 1.75 mm, meeting industry standards for 3D printing. Adjustments to the hot end temperature and motor speed were made to optimize extrusion quality.

### **Throughput**

The machine successfully processed approximately 5 PET bottles per hour. This rate could be improved with automated feeding mechanisms.

### **Reliability**

The system operated continuously for several hours without overheating or mechanical failures. Periodic cleaning of the hot end and gears was required to maintain efficiency.

### **User Feedback**

Users found the machine intuitive to operate, with clear instructions displayed on the graphical LCD. Minor adjustments were needed for first-time use, but overall, the system performed reliably.

## **Challenges and Solutions**

### **Challenges**

* **Uneven Extrusion**: Initial tests showed inconsistencies in filament diameter due to variable feeding speeds.
* **Thermal Issues**: The hot end occasionally overheated, causing clogging and uneven flow.
* **Assembly Complexity**: Aligning components and ensuring secure connections proved challenging.

### **Solutions**

* Improved calibration of the hot end and motor control.
* Added a cooling system to stabilize the hot end’s temperature.
* Enhanced design tolerances for easier assembly.
* Implemented a filament diameter sensor to monitor output consistency in real-time.

## **Conclusion and Future Work**

This project successfully demonstrated the feasibility of converting PET bottles into 3D printing filament. The machine’s design and functionality met the initial objectives. Key achievements include:

* Development of a cost-effective and reliable filament maker.
* Production of consistent, high-quality filament suitable for a variety of 3D printing applications.

### **Future Work**

* **Automation**: Integrate an automated bottle shredding and feeding mechanism.
* **Filament Monitoring**: Add sensors for real-time quality control.
* **Enhanced Throughput**: Optimize the extrusion process to increase production speed.
* **User Interface**: Develop a more advanced interface for enhanced user control and monitoring.

## **References**

1. Instructables. "Turn PET Bottles Into 3D Printer Filament." Available at: <https://www.instructables.com/Turn-PET-Bottles-Into-3D-Printer-Filament/>
2. Printables. "PET Filament Machine." Available at: <https://www.printables.com/model/356919-pet-filament-machine>
3. Google Ad Services. "PET Filament Machine Ad." Available at: <https://www.googleadservices.com/pagead/aclk?sa=L&ai=DChcSEwj88am4qsGKAxVWe0ECHZQtCBQYABABGgJ3cw&ae=2&aspm=1&co=1&ase=5&gclid=Cj0KCQiA1Km7BhC9ARIsAFZfEIu-5eyOU0simKTbdL7eZ8ZzCFITChOpE91RGBUlv5M_srDbytva8F0aAqzJEALw_wcB&ohost=www.google.com&cid=CAESVuD271OxTJ2YEXEJiTBx-8Tm7NsIb-xE0LnNeTWi7_qiL5E2oJlXo4tN491t5EPIvvUnlt-suRNS-zQSi6l8q7lyDN6tdXcWp4TSXzTiISdZtL8AA6n1&sig=AOD64_2KMuUg9S-q3-cmjQ5kFzO9a_2ajQ&q&adurl&ved=2ahUKEwiu6qW4qsGKAxXUVKQEHYIoASEQ0Qx6BAgLEAE>
4. Google Ad Services. "PET Filament Ad." Available at: <https://www.googleadservices.com/pagead/aclk?sa=L&ai=DChcSEwj88am4qsGKAxVWe0ECHZQtCBQYABAAGgJ3cw&ae=2&aspm=1&co=1&ase=5&gclid=Cj0KCQiA1Km7BhC9ARIsAFZfEIv-wUBj3_YbCfdRKRMbz4vS3s8OcUJw3dJP1O9wxyPvWvuFG62PrCoaAgGoEALw_wcB&ohost=www.google.com&cid=CAESVuD271OxTJ2YEXEJiTBx-8Tm7NsIb-xE0LnNeTWi7_qiL5E2oJlXo4tN491t5EPIvvUnlt-suRNS-zQSi6l8q7lyDN6tdXcWp4TSXzTiISdZtL8AA6n1&sig=AOD64_31Z46lk6Qwk1qV0pKIihBSiN3Sdw&q&adurl&ved=2ahUKEwiu6qW4qsGKAxXUVKQEHYIoASEQ0Qx6BAgNEAE>
5. Thingiverse. "PET Filament Machine Model." Available at: <https://www.thingiverse.com/thing:6220558>
6. YouTube. "PET Bottle to Filament Tutorial." Available at: <https://youtu.be/PLiHF8iA8iA?si=umRvbHKQqSuvEbeM>